Flowmap Progress Report  Model
06-17-2011     10:31:31

----------------------------------------
Model parameters
Model Category: Relocation
Model Type: Worst Case Optimisation
Movable Locations: C2FIJOS
Fixed Locations: [None]
Excluded locations: [None]
Weight: POBLACIO
Maximum Distance: [None]
Result Field: SMIMX2I
----------------------------------------
Relocation model: round 1

Accessibility Statistics:
Stable service centers: 1 (out of 2)
Worst case travel impedance: 12091
Average Worst case travel impedance: 11075.14

----------------------------------------
Relocation model: round 2

Accessibility Statistics:
Stable service centers: 1 (out of 2)
Worst case travel impedance: 10294.73
Average Worst case travel impedance: 10177.01

----------------------------------------
Relocation model: round 3

Accessibility Statistics:
Stable service centers: 2 (out of 2)
Worst case travel impedance: 10294.73
Average Worst case travel impedance: 9205.07

Optimal supply location set is stored in 
File: D:\SIGAP\PARTE2\UNIDAD6\DATOS\Siglandia\SiglandiaFM\MUNICIP1.DBF
Field: SMIMX2I (>0)
Ready running Worst Case Optimisation model
   Model run ended successfully!
