Flowmap Progress Report  Model
05-17-2011     17:37:53

----------------------------------------
Model parameters
Model Category: Combination
Model Type: Combination - Best Effect on Average Distance
Partial Solution: [None]
Excluded locations: [None]
Weight: ALUMN
Maximum Distance: [None]
Selection Method (in case of equal scores only): One at Random from list
Stop Criterion: TOP3
Result Field: PM3C_ER
Total Demand: 1331.99609375


========================================
Expansion model: round 1
Average distance range: 1758,72->946,32
Label new supply location(s): 531
Latest supply location was selected out of 8 equal candidates
Total number of (additional) supply locations: 1
Number of client locations served: 998/ 1000

========================================
Expansion model: round 2
Improvement in average distance: 946,32->770,52
Label new supply location(s): 490
Latest supply location was selected out of 2 equal candidates

----------------------------------------
Start Relocation Model
Relocation model: round 1

Accessibility Statistics:
Stable service centers: 0 (out of 2)
Mean average travel impedance: 770,53
----------------------------------------
Relocation model: round 2

Accessibility Statistics:
Stable service centers: 0 (out of 2)
Mean average travel impedance: 717,37
----------------------------------------
Relocation model: round 3

Accessibility Statistics:
Stable service centers: 2 (out of 2)
Mean average travel impedance: 709,69
Labels of current supply locations: 484/516
End Relocation Model
----------------------------------------
Total number of (additional) supply locations: 2
Number of client locations served: 996/ 1000

========================================
Expansion model: round 3
Improvement in average distance: 709,68->609,48
Label new supply location(s): 81
Latest supply location was selected out of 2 equal candidates

----------------------------------------
Start Relocation Model
Relocation model: round 1

Accessibility Statistics:
Stable service centers: 0 (out of 3)
Mean average travel impedance: 609,48
----------------------------------------
Relocation model: round 2

Accessibility Statistics:
Stable service centers: 0 (out of 3)
Mean average travel impedance: 574,44
----------------------------------------
Relocation model: round 3

Accessibility Statistics:
Stable service centers: 2 (out of 3)
Mean average travel impedance: 567,24
----------------------------------------
Relocation model: round 4

Accessibility Statistics:
Stable service centers: 3 (out of 3)
Mean average travel impedance: 567,24
Labels of current supply locations: 145/676/708
End Relocation Model
----------------------------------------
Total number of (additional) supply locations: 3
Number of client locations served: 994/ 1000

!!!Model run finished because:
!!!Requested number of best locations identified!!!

Top 3 supply locations found 
Note: 3 arbitrary selections in expansion model

(Added) supply location ranking is stored in 
File: F:\USB\Tra\bajadensidad1\FM_BD\BUFFBAJ1.DBF
Field: PM3C_ER (rank number)
Ready running Combination - Best Effect on Average Distance model
   Model run ended successfully!
